WB-350 Factory Reset.

Turn machine ON. **There should not be any tire/rim on shaft.**

Press the following sequence of buttons to do a Factory Code Reset.

1. Press Home button



1. Press DIS + button



**Your screen will now display “SET UP”**

A machine with a display and a screen

Description automatically generated with medium confidence

1. Press House 2 Times

A yellow button with a black symbol on it

Description automatically generated

**Your screen will now display “POS” and “some number”**

A machine with a display and buttons

Description automatically generated

1. Rotate shaft until “111” appears in the right window.

A close up of a device

Description automatically generated

1. Hit “C” button.

A yellow button with a black letter on it

Description automatically generated

1. Rotate shaft until “55” appears in the right window.

A machine with a screen and buttons

Description automatically generated

1. Hit “C” button.

A yellow button with a black letter on it

Description automatically generated

1. Rotate shaft until “111” appears in the right window.

A close up of a device

Description automatically generated

1. Hit “C” button.

A yellow button with a black letter on it

Description automatically generated

**Your screen will now display “COD” and “Set”**

A machine with a display and buttons

Description automatically generated

1. Press Home key

A yellow button with a black symbol on it

Description automatically generated

**Your screen will display “some number” on both sides**

A close up of a machine

Description automatically generated

1. Press DIS + repeatedly until “46” appears in the left window. Press home key.

A yellow button with a black symbol on it

Description automatically generated

**Your screen will now display “B-A” and “some number”**

A machine with a display and buttons

Description automatically generated with medium confidence

1. Pull Distance Gauge out and put to Flange – note distance on distance gauge. **The number on the right must match the number noted on the distance gauge.**

**A hand holding a tape measure

Description automatically generated**

1. Change the number on the right by pressing DIS + or DIS –. **The number on the right must match the number noted on the distance gauge.**

A yellow buttons with black text

Description automatically generated

1. Then press Home key.

A yellow button with a black symbol on it

Description automatically generated

**Your screen will now display “EL1” “005”**

A close-up of a machine

Description automatically generated

1. Use DIS + or DIS – to change the number on the right to show 005 (in the unit of Gram) or 007 (in the unit of Ounce)

A yellow buttons with black text

Description automatically generated

1. Press Home key.

A yellow button with a black symbol on it

Description automatically generated

**Your Screen will now display “Tur” “OFF”**

A close up of a machine

Description automatically generated

1. Press home key again

A yellow button with a black symbol on it

Description automatically generated

**You will now hear a series of Beeps**

1. Turn the machine off and back on.

**YOU HAVE COMPLETED FACTORY RESET**

------------------------------------------------------------------------------------